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Product Specification
100G QSFP28 2km CWDM4 Transceivers
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FEATURES
· Compliant with 100G CWDM4 MSA Specification
· Uncooled 4x25Gb/s CWDM transmitter
· Wide Operating Temperature(0°C~70°C)
· Maximum link length of 2km via Single Mode Fiber (SMF)


APPLICATIONS
· Data Center Backbone
· Ethernet Switches
· High-speed Servers
· High-performance Computing Clusters
· SAN, Routers, Hubs, Load Balancer
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ABSOLUTE MAXIMUM RATINGS
	Parameter
	Symbol
	Conditions
	Min.
	Max.
	Unit

	Storage Temperature
	TStorage
	
	-40
	+85
	°C

	Relative Humidity
	RH
	
	0
	+85
	%



RECOMMENDED OPERATING CONDITIONS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Case Temperature
	TC
	
	0
	
	70
	°C

	Power Supply Voltage
	VCC
	
	3.135
	3.3
	3.465
	V

	Signaling Rate each Channel
	
	
	
	25.78125
	
	Gbps

	Supply Noise Rejection
	
	
	---
	---
	100
	mV

	Receiver Differential Data Output
	
	
	---
	100
	
	Ohm

	Operating Distance
	D
	
	---
	---
	2
	km




























ELECTRICAL CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Power Consumption
	
	
	
	
	3.5
	W

	Supply Current
	Icc
	
	
	
	1050
	mA




TRANSMITTER CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Signaling rate, each lane (range)
	GBb
	
	
	25.78125 
	
	GBb

	Center Wavelength
	λ0
	
	1264.5
	
	1277.5
	nm

	
	λ1
	
	1284.5
	
	1297.5
	nm

	
	λ2
	
	1304.5
	
	1317.5
	nm

	
	λ3
	
	1324.5
	
	1337.5
	nm

	Side-mode suppression ratio 
	SMSR
	
	30
	
	
	dB

	Total average launch power
	
	
	
	
	8.5
	dBm

	Average launch power, each lane
	Pf
	
	-6.5
	
	2.5
	dBm

	Optical Modulation Amplitude (OMA), each lane
	TxOMA
	
	-5
	
	2.5
	dBm

	Transmitter and Dispersion Penalty
	TDP
	
	
	
	3
	dB

	Launch power in OMA minus TDP, each lane
	Tx-TDP
	
	-5
	
	
	dBm

	Average launch power of OFF transmitter, each lane
	
	
	
	
	-30
	dBm

	Extinction ratio
	ER
	
	3.5
	
	
	dB

	Optical return loss tolerance
	
	
	
	
	20
	dB

	Transmitter reflectance
	
	
	
	
	-12
	dB
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RECEIVER CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Signaling rate, each lane (range)
	GBb
	
	
	25.78125 
	
	GBb

	Center Wavelength
	λ0
	
	1264.5
	
	1277.5
	nm

	
	λ1
	
	1284.5
	
	1297.5
	nm

	
	λ2
	
	1304.5
	
	1317.5
	nm

	
	λ3
	
	1324.5
	
	1337.5
	nm

	Damage threshold
	
	
	3.5
	
	
	dBm

	Average power at receiver input, each lane
	
	
	-10
	
	2.5
	dBm

	Receive power, each lane (OMA)
	
	
	
	
	2.5
	dBm

	Receiver reflectance
	
	
	
	
	-26
	dB

	Receiver sensitivity (OMA)
	SOMA
	BER@5e-5
	
	
	-10
	dBm

	LOS Assert 
	LOSA
	
	-24
	
	
	dBm

	LOS De-Assert 
	LOSD
	
	
	
	-11.6
	dBm

	LOS Hysteresis
	
	
	0.5
	
	6
	dB



PIN ASSIGNMENT  
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PIN DESCRIPTION  

	PIN
	Logic
	Symbol
	Name/Description
	Note

	1
	 
	GND
	Ground
	

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input
	

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data output
	

	4
	 
	GND
	Ground
	

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input
	

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data output
	

	7
	 
	GND
	Ground
	

	8
	LVTTL-I
	ModSelL
	Module Select
	

	9
	LVTTL-I
	ResetL
	Module Reset
	

	10
	 
	VccRx
	﹢3.3V Power Supply Receiver
	

	11
	LVCMOS-I/O
	SCL
	2-Wire Serial Interface Clock
	

	12
	LVCMOS-I/O
	SDA
	2-Wire Serial Interface Data
	

	13
	 
	GND
	Ground
	

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data Output
	

	15
	CML-O 
	Rx3n 
	Receiver Inverted Data Output 
	

	16
	 
	GND 
	Ground 
	

	17
	CML-O 
	Rx1p 
	Receiver Non-Inverted Data Output 
	

	18
	CML-O 
	Rx1n 
	Receiver Inverted Data Output 
	

	19
	 
	GND 
	Ground 
	

	20
	 
	GND 
	Ground 
	

	21
	CML-O 
	Rx2n 
	Receiver Inverted Data Output 
	

	22
	CML-O 
	Rx2p 
	Receiver Non-Inverted Data Output 
	

	23
	 
	GND 
	Ground 
	

	24
	CML-O 
	Rx4n 
	Receiver Inverted Data Output 
	

	25
	CML-O 
	Rx4p 
	Receiver Non-Inverted Data Output 
	

	26
	 
	GND 
	Ground 
	

	27
	LVTTL-O 
	ModPrsL 
	Module Present 
	

	28
	LVTTL-O 
	IntL 
	Interrupt 
	

	29
	 
	VccTx 
	+3.3 V Power Supply transmitter 
	

	30
	 
	Vcc1 
	+3.3 V Power Supply 
	

	31
	LVTTL-I 
	LPMode 
	Low Power Mode 
	

	32
	 
	GND 
	Ground 
	

	33
	CML-I 
	Tx3p 
	Transmitter Non-Inverted Data Input 
	

	34
	CML-I 
	Tx3n 
	Transmitter Inverted Data Output 
	

	35
	 
	GND 
	Ground 
	

	36
	CML-I 
	Tx1p 
	Transmitter Non-Inverted Data Input 
	

	37
	CML-I 
	Tx1n 
	Transmitter Inverted Data Output 
	

	38
	 
	GND 
	Ground 
	




OUTLINE DIMENSIONS  
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Digital Diagnostic Monitor Accuracy
The following characteristics are defined over recommended operating conditions

	Parameter
	Accuracy
	Unit

	Internally measured transceiver temperature
	+/-3
	deg.C

	Internally measured transceiver supply voltage
	+/-3
	%

	Measured Tx bias current
	+/-10
	%

	[bookmark: _GoBack]Measured Tx output power
	+/-3
	dB

	Measured Rx received average optical power
	+/-3
	dB



Contact:
Wuhan Jiuhong Optics Technology Co., Ltd.
TEL: 86-13476016116
E-mail：grace@jh-optics.com
Web：www.jh-optics.com
Address：
Building 1, 4th Floor, Yunqi Free Trade Innovation Port, Donghu Comprehensive Bonded Zone,Donghu High-tech Zone, Wuhan City
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