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    200G QSFP-DD Direct Attach Cable  Datasheet

General  Description

QSFP-DD passive copper cable assembly feature eight differential copper pairs,providing four data transmission channels at speeds up to 28Gbps per channel,and meets 200G Ethernet and InfiniBand Enhanced Data Rate(EDR) requirements.Available in a broad rang of wire gages-from 28AWG through 30AWG-this 200G copper cable assembly features low insertion loss and low cross talk.
Features and Benefits

·  Compatible with IEEE 802.3bj and IEEE 802.3cd
·    Supports aggregate data rates of 200Gbps
·  Optimized construction to minimize insertion loss and cross talk 
·  Pull-to-release slide latch design
·  28AWG through 30AWG cable
·  Straight and break out assembly configurations available
·   Customized cable braid termination limits EMI radiation   
·   Customizable EEPROM mapping for cable signature
·   RoHS omplia

Product Applications

· Switches,servers and routers
· Data Center networks
· Storage area networks
· High performance computing
· Telecommunication and wireless infrastructure
· Medical diagnostics and networking
· Test and measurement equipment

Industry  Standards

· 200G Ethernet(IEEE 802.3cd)
· InfiniBand EDR 





High Speed Characteristics
	Parameter
	Symbol
	Min
	Typical
	Max
	Unit
	Note

	Differential Impedance
	TDR
	90
	100
	110
	Ώ
	

	Insertion loss
	SDD21
	-16.06
	
	-8
	dB
	At 13.28 GHz

	Differential Return Loss
	SDD11
SDD22
	-12.45
	
	See 1
	dB
	At 0.05 to 4.1 GHz

	
	
	-3.12
	
	See 2
	dB
	At 4.1 to 19 GHz

	Common-mode to common-mode output return loss
	SCC11
SCC22
	
	
	-2
	dB
	At 0.2 to 19 GHz

	Differential to common-mode
return loss
	SCD11
SCD22
	-12
	
	See 3
	dB
	At 0.01 to 12.89 GHz

	
	
	-10.58
	
	See 4
	
	At 12.89 to 19 GHz

	Differential to common Mode
Conversion Loss
	SCD21-IL
	
	
	-10
	dB
	At 0.01 to 12.89 GHz

	
	
	
	
	See 5
	
	At 12.89 to 15.7 GHz

	
	
	
	
	-6.3
	
	At 15.7 to 19 GHz

	Notes:
1. Reflection Coefficient given by equation SDD11(dB) < -16.5 + 2 × SQRT(f ), with f in GHz
2. Reflection Coefficient given by equation SDD11(dB) < -10.66 + 14 × log10(f/5.5), with f in GHz
3. Reflection Coefficient given by equation SCD11(dB) < -22 + (20/25.78)*f, with f in GHz
4. Reflection Coefficient given by equation SCD11(dB) < -15 + (6/25.78)*f, with f in GHz
5. Reflection Coefficient given by equation SCD21(dB) < -27 + (29/22)*f, with f in GHz




Pin Descriptions
QSFP-DD Pin Function Definition

	Pin
	Logic
	Symbol
	Description

	1
	
	GND
	Ground

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data Input

	4
	
	GND
	Ground

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data Input

	7
	
	GND
	Ground

	8
	LVTTL-I
	ModSelL
	Module Select

	9
	LVTTL-I
	ResetL
	Module Reset

	10
	
	Vcc Rx
	+3.3V Power Supply Receiver

	11
	LVCMOS-
	SCL
	2-wire serial interface clock

	
	I/O
	
	

	12
	LVCMOS-
	SDA
	2-wire serial interface data

	
	I/O
	
	

	13
	
	GND
	Ground

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data Output

	15
	CML-O
	Rx3n
	Receiver Inverted Data Output

	16
	
	GND
	Ground

	17
	CML-O
	Rx1p
	Receiver Non-Inverted Data Output

	18
	CML-O
	Rx1n
	Receiver Inverted Data Output

	19
	
	GND
	Ground

	20
	
	GND
	Ground

	21
	CML-O
	Rx2n
	Receiver Inverted Data Output

	22
	CML-O
	Rx2p
	Receiver Non-Inverted Data Output

	23
	
	GND
	Ground

	24
	CML-O
	Rx4n
	Receiver Inverted Data Output

	25
	CML-O
	Rx4p
	Receiver Non-Inverted Data Output

	26
	
	GND
	Ground

	27
	LVTTL-O
	ModPrsL
	Module Present

	28
	LVTTL-O
	IntL
	Interrupt

	29
	
	Vcc Tx
	+3.3V Power supply transmitter

	30
	
	Vcc1
	+3.3V Power supply

	31
	LVTTL-I
	LPMode
	Low Power Mode

	32
	
	GND
	Ground

	33
	CML-I
	Tx3p
	Transmitter Non-Inverted Data Input

	34
	CML-I
	Tx3n
	Transmitter Inverted Data Input

	35
	
	GND
	Ground

	36
	CML-I
	Tx1p
	Transmitter Non-Inverted Data Input

	37
	CML-I
	Tx1n
	Transmitter Inverted Data Input

	38
	
	GND
	Ground

	39
	
	GND
	Ground

	40
	CML-I
	Tx6n
	Transmitter Inverted Data Input

	41
	CML-I
	Tx6p
	Transmitter Non-Inverted Data Input

	42
	
	GND
	Ground

	43
	CML-I
	Tx8n
	Transmitter Inverted Data Input

	44
	CML-I
	Tx8p
	Transmitter Non-Inverted Data Input

	45
	
	GND
	Ground

	46
	
	Reserved
	

	47
	
	VS1
	

	48
	
	VccRx1
	+3.3V Power supply

	49
	
	VS2
	

	50
	
	VS3
	

	51
	
	GND
	Ground

	52
	CML-O
	Rx7p
	Receiver Non-Inverted Data Output

	53
	CML-O
	Rx7n
	Receiver Inverted Data Output

	54
	
	GND
	Ground

	55
	CML-O
	Rx5p
	Receiver Non-Inverted Data Output

	56
	CML-O
	Rx5n
	Receiver Inverted Data Output

	57
	
	GND
	Ground

	58
	
	GND
	Ground

	59
	CML-O
	Rx6n
	Receiver Inverted Data Output

	60
	CML-O
	Rx6p
	Receiver Non-Inverted Data Output

	61
	
	GND
	Ground

	62
	CML-O
	Rx8n
	Receiver Inverted Data Output

	63
	CML-O
	Rx8p
	Receiver Non-Inverted Data Output

	64
	
	GND
	Ground

	65
	
	NC
	

	66
	
	Reserved
	

	67
	
	VccTx1
	+3.3V Power supply

	68
	
	VCC2
	+3.3V Power supply

	69
	
	Reserved
	

	70
	
	GND
	Ground

	71
	CML-I
	Tx7p
	Transmitter Non-Inverted Data Input

	72
	CML-I
	Tx7n
	Transmitter Inverted Data Input

	73
	
	GND
	Ground

	74
	CML-I
	Tx5p
	Transmitter Non-Inverted Data Input

	75
	CML-I
	Tx5n
	Transmitter Inverted Data Input

	76
	
	GND
	Ground
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Mechanical Specifications
The connector is compatible with the QSFP-DD specification.
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	Length (m)
	Cable AWG

	1.5
	30

	2.5
	28



Regulatory Compliance

	Feature
	Test Method
	Performance

	Electrostatic Discharge (ESD) to the Electrical Pins
	
MIL-STD-883C Method 3015.7
	
Class 1(>2000 Volts)

	Electromagnetic Interference(EMI)
	FCC Class B
	Compliant with Standards

	
	CENELEC EN55022 Class B
	

	
	CISPR22 ITE Class B
	

	
RF Immunity(RFI)
	
IEC61000-4-3
	Typically Show no Measurable Effect from a 10V/m Field Swept from 80 to 1000MHz

	RoHS Compliance
	RoHS Directive 2011/65/EU and it's Amendment Directives （EU） 2015/863
	RoHS （EU）2015/863 compliant

	REACH Compliance
	REACH  Regulation (EC) No 1907/2006
	REACH (EC) No 1907/2006 compliant


Contact:
Wuhan Jiuhong Optics Technology Co., Ltd.
TEL: 86-13476016116
E-mail：grace@jh-optics.com
Web：www.jh-optics.com
[bookmark: _GoBack]Address：
Building 1, 4th Floor, Yunqi Free Trade Innovation Port, Donghu Comprehensive Bonded Zone,Donghu High-tech Zone, Wuhan City

© Wuhan Jiuhong Optics Technology Co., Ltd.
Web: www.jh-optics.com
Email: grace@jh-optics.com
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