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200G QSFP-DD-2X100G QSFP28 Direct Attach Cable

Features and Benefits

·  Compatible with IEEE 802.3bj and IEEE 802.3cd
·    Supports aggregate data rates of 200Gbps
·  Optimized construction to minimize insertion loss and cross talk 
·  Pull-to-release slide latch design
·  28AWG through 30AWG cable
·  Straight and break out assembly configurations available
·   Customized cable braid termination limits EMI radiation   
·   Customizable EEPROM mapping for cable signature
·   RoHS Compliance

Product Applications

· Switches, servers and routers
· Data Center networks
· Storage area networks
· High performance computing
· Telecommunication and wireless infrastructure
· Medical diagnostics and networking
· Test and measurement equipment

Industry Standards

· 200G Ethernet(IEEE 802.3cd)
· InfiniBand EDR 

General  Description

QSFP-DD_2XQSFP28 passive copper cable assembly feature eight differential copper pairs, providing four data transmission channels at speeds up to 28Gbps per channel and meets 200G Ethernet and InfiniBand Enhanced Data Rate(EDR) requirements. Available in a broad rang of wire gages-from 28AWG through 30AWG-this 200G copper cable assembly features low insertion loss and low cross talk.





High Speed Characteristics
	Parameter
	Symbol
	Min
	Typical
	Max
	Unit
	Note

	Differential Impedance
	TDR
	90
	100
	110
	Ώ
	

	Insertion loss
	SDD21
	-22.48
	
	
	dB
	At 12.89 GHz

	Differential Return Loss
	SDD11
SDD22
	
	
	See 1
	dB
	At 0.05 to 4.1 GHz

	
	
	
	
	See 2
	dB
	At 4.1 to 19 GHz

	Common-mode to common-mode output return loss
	SCC11
SCC22
	
	
	-2
	dB
	At 0.2 to 19 GHz

	Differential to common-mode
return loss
	SCD11
SCD22
	
	
	See 3
	dB
	At 0.01 to 12.89 GHz

	
	
	
	
	See 4
	
	At 12.89 to 19 GHz

	Differential to common Mode
Conversion Loss
	SCD21-IL
	
	
	-10
	dB
	At 0.01 to 12.89 GHz

	
	
	
	
	See 5
	
	At 12.89 to 15.7 GHz

	
	
	
	
	-6.3
	
	At 15.7 to 19 GHz

	Notes:
1. Reflection Coefficient given by equation SDD11(dB) < -16.5 + 2 × SQRT(f ), with f in GHz
2. Reflection Coefficient given by equation SDD11(dB) < -10.66 + 14 × log10(f/5.5), with f in GHz
3. Reflection Coefficient given by equation SCD11(dB) < -22 + (20/25.78)*f, with f in GHz
4. Reflection Coefficient given by equation SCD11(dB) < -15 + (6/25.78)*f, with f in GHz
5. Reflection Coefficient given by equation SCD21(dB) < -27 + (29/22)*f, with f in GHz




Pin Descriptions
QSFP-DD Pin Function Definition

	Pin
	Logic
	Symbol
	Description

	1
	
	GND
	Ground

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data Input

	4
	
	GND
	Ground

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data Input

	7
	
	GND
	Ground

	8
	LVTTL-I
	ModSelL
	Module Select

	9
	LVTTL-I
	ResetL
	Module Reset

	10
	
	Vcc Rx
	+3.3V Power Supply Receiver

	11
	LVCMOS-
	SCL
	2-wire serial interface clock

	
	I/O
	
	

	12
	LVCMOS-
	SDA
	2-wire serial interface data

	
	I/O
	
	

	13
	
	GND
	Ground

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data Output

	15
	CML-O
	Rx3n
	Receiver Inverted Data Output

	16
	
	GND
	Ground

	17
	CML-O
	Rx1p
	Receiver Non-Inverted Data Output

	18
	CML-O
	Rx1n
	Receiver Inverted Data Output

	19
	
	GND
	Ground

	20
	
	GND
	Ground

	21
	CML-O
	Rx2n
	Receiver Inverted Data Output

	22
	CML-O
	Rx2p
	Receiver Non-Inverted Data Output

	23
	
	GND
	Ground

	24
	CML-O
	Rx4n
	Receiver Inverted Data Output

	25
	CML-O
	Rx4p
	Receiver Non-Inverted Data Output

	26
	
	GND
	Ground

	27
	LVTTL-O
	ModPrsL
	Module Present

	28
	LVTTL-O
	IntL
	Interrupt

	29
	
	Vcc Tx
	+3.3V Power supply transmitter

	30
	
	Vcc1
	+3.3V Power supply

	31
	LVTTL-I
	LPMode
	Low Power Mode

	32
	
	GND
	Ground

	33
	CML-I
	Tx3p
	Transmitter Non-Inverted Data Input

	34
	CML-I
	Tx3n
	Transmitter Inverted Data Input

	35
	
	GND
	Ground

	36
	CML-I
	Tx1p
	Transmitter Non-Inverted Data Input

	37
	CML-I
	Tx1n
	Transmitter Inverted Data Input

	38
	
	GND
	Ground

	39
	
	GND
	Ground

	40
	CML-I
	Tx6n
	Transmitter Inverted Data Input

	41
	CML-I
	Tx6p
	Transmitter Non-Inverted Data Input

	42
	
	GND
	Ground

	43
	CML-I
	Tx8n
	Transmitter Inverted Data Input

	44
	CML-I
	Tx8p
	Transmitter Non-Inverted Data Input

	45
	
	GND
	Ground

	46
	
	Reserved
	

	47
	
	VS1
	

	48
	
	VccRx1
	+3.3V Power supply

	49
	
	VS2
	

	50
	
	VS3
	

	51
	
	GND
	Ground

	52
	CML-O
	Rx7p
	Receiver Non-Inverted Data Output

	53
	CML-O
	Rx7n
	Receiver Inverted Data Output

	54
	
	GND
	Ground

	55
	CML-O
	Rx5p
	Receiver Non-Inverted Data Output

	56
	CML-O
	Rx5n
	Receiver Inverted Data Output

	57
	
	GND
	Ground

	58
	
	GND
	Ground

	59
	CML-O
	Rx6n
	Receiver Inverted Data Output

	60
	CML-O
	Rx6p
	Receiver Non-Inverted Data Output

	61
	
	GND
	Ground

	62
	CML-O
	Rx8n
	Receiver Inverted Data Output

	63
	CML-O
	Rx8p
	Receiver Non-Inverted Data Output

	64
	
	GND
	Ground

	65
	
	NC
	

	66
	
	Reserved
	

	67
	
	VccTx1
	+3.3V Power supply

	68
	
	VCC2
	+3.3V Power supply

	69
	
	Reserved
	

	70
	
	GND
	Ground

	71
	CML-I
	Tx7p
	Transmitter Non-Inverted Data Input

	72
	CML-I
	Tx7n
	Transmitter Inverted Data Input

	73
	
	GND
	Ground

	74
	CML-I
	Tx5p
	Transmitter Non-Inverted Data Input

	75
	CML-I
	Tx5n
	Transmitter Inverted Data Input

	76
	
	GND
	Ground
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	Pin
	Logic
	Symbol
	Description

	1
	
	GND
	Ground

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data Input

	4
	
	GND
	Ground

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data Input

	7
	
	GND
	Ground

	8
	LVTTL-I
	ModSelL
	Module Select

	9
	LVTTL-I
	ResetL
	Module Reset

	10
	
	Vcc Rx
	+3.3V Power Supply Receiver

	11
	LVCMOS-
	SCL
	2-wire serial interface clock

	
	I/O
	
	

	12
	LVCMOS-
	SDA
	2-wire serial interface data

	
	I/O
	
	

	13
	
	GND
	Ground

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data Output

	15
	CML-O
	Rx3n
	Receiver Inverted Data Output

	16
	
	GND
	Ground

	17
	CML-O
	Rx1p
	Receiver Non-Inverted Data Output

	18
	CML-O
	Rx1n
	Receiver Inverted Data Output

	19
	
	GND
	Ground

	20
	
	GND
	Ground

	21
	CML-O
	Rx2n
	Receiver Inverted Data Output

	22
	CML-O
	Rx2p
	Receiver Non-Inverted Data Output

	23
	
	GND
	Ground

	24
	CML-O
	Rx4n
	Receiver Inverted Data Output

	25
	CML-O
	Rx4p
	Receiver Non-Inverted Data Output

	26
	
	GND
	Ground

	27
	LVTTL-O
	ModPrsL
	Module Present

	28
	LVTTL-O
	IntL
	Interrupt

	29
	
	Vcc Tx
	+3.3V Power supply transmitter

	30
	
	Vcc1
	+3.3V Power supply

	31
	LVTTL-I
	LPMode
	Low Power Mode

	32
	
	GND
	Ground

	33
	CML-I
	Tx3p
	Transmitter Non-Inverted Data Input

	34
	CML-I
	Tx3n
	Transmitter Inverted Data Input

	35
	
	GND
	Ground

	36
	CML-I
	Tx1p
	Transmitter Non-Inverted Data Input

	37
	CML-I
	Tx1n
	Transmitter Inverted Data Input

	38
	
	GND
	Ground
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Mechanical Specifications
The connector is compatible with the QSFP-DD and SFF-8661 specification.
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	Length (m)
	Wire Gauge

	0.5~3
	30AWG

	3~4
	28AWG



Regulatory Compliance

	Feature
	Test Method
	Performance

	Electrostatic Discharge (ESD) to the Electrical Pins
	
MIL-STD-883C Method 3015.7
	
Class 1(>2000 Volts)

	Electromagnetic Interference(EMI)
	FCC Class B
	Compliant with Standards

	
	CENELEC EN55022 Class B
	

	
	CISPR22 ITE Class B
	

	
RF Immunity(RFI)
	
IEC61000-4-3
	Typically Show no Measurable Effect from a 10V/m Field Swept from 80 to 1000MHz

	RoHS Compliance
	RoHS Directive 2011/65/EU and it's Amendment Directives （EU） 2015/863
	RoHS （EU）2015/863 compliant

	REACH Compliance
	REACH  Regulation (EC) No 1907/2006
	REACH (EC) No 1907/2006 compliant
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