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Product Specification
400G QSFP-DD to 4x QSFP56 AOC Transceivers
 
DESCRIPTION

This is 400Gb/s QSFP-DD to 4x QSFP56 active optical cable (AOC).It is compliant with the QSFP-DD MSA Rev5.0 and IEEE 802.3bs, IEEE802.3cm, and Common Management Interface Specification Rev4.0. The AOC is an assembly of eight full-duplex lanes, where each lane is capable of transmitting data at rates up to 53.125Gb/s PAM-4 signal mode.

FEATURES
· [bookmark: OLE_LINK1][bookmark: OLE_LINK3]Data rate up to 425Gb/s (8x PAM4 53Gb/s)
· 850nm VCSEL laser and PIN receiver
· QSFP-DD: High speed I/O electrical interface (400GAUI-8)(CMIS)
· QSFP56: Hot Pluggable QSFP56 form factor（8636）
· I2C interface with integrated Digital Diagnostic Monitoring (DDM)
· Single +3.3V power supply
· QSFP-DD : Power consumption less than 10W per end
· QSFP56 : Power consumption <4.5W
· Low latency time with DSP solution
· Operating case temperature:0~+70°C
· Compliant to RoHS-10

APPLICATION 
· DATA CENTER


Ordering information
	Part Number
	Product Description

	JH-400G-QDD
[bookmark: _GoBack]-Q56-A4-AOC
	400G QSFP-DD to 4x QSFP56 AOC Transceivers, C-TEMP,DSP
xx=01~99,cable length=1m~99m




ABSOLUTE MAXIMUM RATINGS (TC=25°C, UNLESS OTHERWISE NOTED)
Stresses in excess of the absolute maximum ratings can cause permanent damage to the device. These are absolute stress ratings only. Functional operation of the device is not implied at these or any other conditions in excess of those given in the operational sections of the data sheet. Exposure to absolute maximum ratings will cause permanent damage and/or adversely affect device reliability.
	Parameter
	Symbol
	Min
	Typical
	Max
	Unit
	Notes

	Storage Temperature
	TS
	-40
	-
	+85
	ºC
	

	Maximum Supply Voltage
	Vcc
	-0.5
	-
	4.0
	V
	

	Operating Relative Humidity
	RH
	15
	-
	+85
	%
	



RECOMMENDED OPERATING CONDITIONS
	Parameter
	Symbol
	Min
	Typical
	Max
	Unit
	Notes

	Operating Case temperature
	Tc
	0
	-
	+70
	ºC
	

	Supply Voltage
	Vcc
	3.13
	3.3
	3.47
	V
	

	Power Supply Current
	Icc
	-
	-
	3
	A
	

	Power Consumption (per end)
	
	-
	-
	10
	W
	QSFP-DD

	Power Consumption (per end)
	
	-
	-
	4.5
	W
	QSFP56

	Data Rate (per lane)
	
	-
	53.125
	-
	Gb/s
	


QSFP-DD PIN DESCRIPTIONS
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[image: ]
	Pad 
	Logic
	Symbol
	Description
	Plug Seq4
	Notes

	1
	
	GND 
	Ground 
	1B
	1

	2
	CML-I 
	Tx2n 
	Transmitter Inverted Data Input 
	3B
	

	3
	CML-I 
	Tx2p 
	Transmitter Non-Inverted Data Input 
	3B
	

	4
	
	GND 
	Ground 
	1B
	1

	5
	CML-I 
	Tx4n 
	Transmitter Inverted Data Input 
	3B
	

	6
	CML-I 
	Tx4p 
	Transmitter Non-Inverted Data Input 
	3B
	

	7
	
	GND 
	Ground 
	1B
	1

	8
	LVTTL-I 
	ModSelL 
	Module Select. 
	3B
	

	9
	LVTTL-I 
	ResetL 
	Module Reset. 
	3B
	

	10
	
	VccRx 
	+3.3V Power Supply Receiver 
	2B
	2

	11
	LVCMOS-I/O 
	SCL 
	2-wire serial interface clock 
	3B
	

	12
	LVCMOS-I/O 
	SDA 
	2-wire serial interface data 
	3B
	

	13
	
	GND 
	Ground 
	1B
	1

	14
	CML-O 
	Rx3p 
	Receiver Non-Inverted Data Output 
	3B
	

	15
	CML-O 
	Rx3n 
	Receiver Inverted Data Output 
	3B
	

	16
	
	GND 
	Ground 
	1B
	1

	17
	CML-O 
	Rx1p 
	Receiver Non-Inverted Data Output 
	3B
	

	18
	CML-O 
	Rx1n 
	Receiver Inverted Data Output 
	3B
	

	19
	
	GND 
	Ground 
	1B
	1

	20
	
	GND 
	Ground 
	1B
	1

	21
	CML-O 
	Rx2n 
	Receiver Inverted Data Output 
	3B
	

	22
	CML-O 
	Rx2p 
	Receiver Non-Inverted Data Output 
	3B
	

	23
	
	GND 
	Ground 
	1B
	1

	24
	CML-O 
	Rx4n 
	Receiver Inverted Data Output 
	3B
	

	25
	CML-O 
	Rx4p 
	Receiver Non-Inverted Data Output 
	3B
	

	26
	
	GND 
	Ground 
	1B
	1

	27
	LVTTL-O 
	ModPrsL 
	Module Present. 
	3B
	

	28
	LVTTL-O 
	IntL 
	Interrupt. 
	3B
	

	29
	
	VccTx 
	+3.3V Power supply transmitter 
	2B
	2

	30
	
	Vcc1 
	+3.3V Power supply 
	2B
	2

	31
	LVTTL-I 
	LPMode 
	Low Power Mode
	3B
	

	32
	
	GND 
	Ground 
	1B
	1

	33
	CML-I 
	Tx3p 
	Transmitter Non-Inverted Data Input 
	3B
	

	34
	CML-I 
	Tx3n 
	Transmitter Inverted Data Input 
	3B
	

	35
	
	GND 
	Ground 
	1B
	1

	36
	CML-I 
	Tx1p 
	Transmitter Non-Inverted Data Input 
	3B
	

	37
	CML-I 
	Tx1n 
	Transmitter Inverted Data Input 
	3B
	

	38
	
	GND 
	Ground 
	1B
	1

	39
	
	GND 
	Ground 
	1A
	1

	40
	CML-I 
	Tx6n 
	Transmitter Inverted Data Input 
	3A
	

	41
	CML-I 
	Tx6p 
	Transmitter Non-Inverted Data Input 
	3A
	

	42
	
	GND 
	Ground 
	1A
	1

	43
	CML-I 
	Tx8n 
	Transmitter Inverted Data Input 
	3A
	

	44
	CML-I 
	Tx8p 
	Transmitter Non-Inverted Data Input 
	3A
	

	45
	
	GND 
	Ground 
	1A
	1

	46
	
	Reserved 
	For future use 
	3A
	3

	47
	
	VS1 
	Module Vendor Specific 1 
	3A
	3

	48
	
	VccRx1 
	3.3V Power Supply 
	2A
	2

	49
	
	VS2 
	Module Vendor Specific 2 
	3A
	

	50
	
	VS3 
	Module Vendor Specific 3 
	3A
	

	51
	
	GND 
	Ground 
	1A
	1

	52
	CML-O 
	Rx7p 
	Receiver Non-Inverted Data Output 
	3A
	

	53
	CML-O 
	Rx7n 
	Receiver Inverted Data Output 
	3A
	

	54
	
	GND 
	Ground 
	1A
	1

	55
	CML-O 
	Rx5p 
	Receiver Non-Inverted Data Output 
	3A
	

	56
	CML-O 
	Rx5n 
	Receiver Inverted Data Output 
	3A
	

	57
	
	GND 
	Ground 
	1A
	1

	58
	
	GND 
	Ground 
	1A
	1

	59
	CML-O 
	Rx6n 
	Receiver Inverted Data Output 
	3A
	

	60
	CML-O 
	Rx6p 
	Receiver Non-Inverted Data Output 
	3A
	

	61
	
	GND 
	Ground 
	1A
	1

	62
	CML-O 
	Rx8n 
	Receiver Inverted Data Output 
	3A
	

	63
	CML-O 
	Rx8p 
	Receiver Non-Inverted Data Output 
	3A
	

	64
	
	GND 
	Ground 
	1A
	1

	65
	
	NC 
	No Connect 
	3A
	3

	66
	
	Reserved 
	For future use 
	3A
	3

	67
	
	VccTx1 
	3.3V Power Supply 
	2A
	2

	68
	
	Vcc2 
	3.3V Power Supply 
	2A
	2

	69
	LVTTL-I
	ePPS
	Precision Time Protocol (PTP) reference clock input
	3A
	3

	70
	
	GND 
	Ground 
	1A
	1

	71
	CML-I 
	Tx7p 
	Transmitter Non-Inverted Data Input 
	3A
	

	72
	CML-I 
	Tx7n 
	Transmitter Inverted Data Input 
	3A
	

	73
	
	GND 
	Ground 
	1A
	1

	74
	CML-I 
	Tx5p 
	Transmitter Non-Inverted Data Input 
	3A
	

	75
	CML-I 
	Tx5n 
	Transmitter Inverted Data Input 
	3A
	

	76
	
	GND 
	Ground 
	1A
	1



Notes:
[1] QSFP-DD uses common ground (GND) for all signals and supply (power). All are common within the QSFP-DD module and all module voltages are referenced to this potential unless otherwise noted. Connect these directly to the host board signal-common ground plane.
[2] VccRx, VccRx1, Vcc1, Vcc2, VccTx and VccTx1 shall be applied concurrently. Requirements defined for the host side of the Host Card Edge Connector are listed in Table 7. VccRx, VccRx1, Vcc1, Vcc2, VccTx and VccTx1 may be internally connected within the module in any combination. The connector Vcc pins are each rated for a maximum current of 1000 mA.
[3] All Vendor Specific, Reserved, No Connect and ePPS (if not used) pins may be terminated with 50 Ohms to ground on the host. Pad 65 (No Connect) shall be left unconnected within the module. Vendor specific and Reserved pads shall have an impedance to GND that is greater than 10 kOhms and less than 100 pF.
[4] Plug Sequence specifies the mating sequence of the host connector and module. The sequence is 1A, 2A, 3A, 1B, 2B, 3B (see Figure 2 for pad locations).  Contact sequence A will make, then break contact with additional QSFP-DD pads. Sequence 1A,1B will then occur simultaneously, followed by 2A,2B, followed by 3A, 3B.









QSFP56 PIN DESCRIPTIONS
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	PIN
	Logic
	Symbol
	Name/Description
	Note

	1
	 
	GND
	Ground
	

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input
	

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data output
	

	4
	 
	GND
	Ground
	

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input（not used）
	

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data output（not used）
	

	7
	 
	GND
	Ground
	

	8
	LVTTL-I
	ModSelL
	Module Select
	

	9
	LVTTL-I
	ResetL
	Module Reset
	

	10
	 
	VccRx
	﹢3.3V Power Supply Receiver
	

	11
	LVCMOS-I/O
	SCL
	2-Wire Serial Interface Clock
	

	12
	LVCMOS-I/O
	SDA
	2-Wire Serial Interface Data
	

	13
	 
	GND
	Ground
	

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data Output（not used）
	

	15
	CML-O 
	Rx3n 
	Receiver Inverted Data Output （not used）
	

	16
	 
	GND 
	Ground 
	

	17
	CML-O 
	Rx1p 
	Receiver Non-Inverted Data Output 
	

	18
	CML-O 
	Rx1n 
	Receiver Inverted Data Output 
	

	19
	 
	GND 
	Ground 
	

	20
	 
	GND 
	Ground 
	

	21
	CML-O 
	Rx2n 
	Receiver Inverted Data Output 
	

	22
	CML-O 
	Rx2p 
	Receiver Non-Inverted Data Output 
	

	23
	 
	GND 
	Ground 
	

	24
	CML-O 
	Rx4n 
	Receiver Inverted Data Output （not used）
	

	25
	CML-O 
	Rx4p 
	Receiver Non-Inverted Data Output （not used）
	

	26
	 
	GND 
	Ground 
	

	27
	LVTTL-O 
	ModPrsL 
	Module Present 
	

	28
	LVTTL-O 
	IntL 
	Interrupt 
	

	29
	 
	VccTx 
	+3.3 V Power Supply transmitter 
	

	30
	 
	Vcc1 
	+3.3 V Power Supply 
	

	31
	LVTTL-I 
	LPMode 
	Low Power Mode 
	

	32
	 
	GND 
	Ground 
	

	33
	CML-I 
	Tx3p 
	Transmitter Non-Inverted Data Input （not used）
	

	34
	CML-I 
	Tx3n 
	Transmitter Inverted Data Output （not used）
	

	35
	 
	GND 
	Ground 
	

	36
	CML-I 
	Tx1p 
	Transmitter Non-Inverted Data Input 
	

	37
	CML-I 
	Tx1n 
	Transmitter Inverted Data Output 
	

	38
	 
	GND 
	Ground 
	



DATA RATE SPECIFICATION
	Parameter
	Symbol
	Min
	Typical
	Max
	Units
	Notes

	Bit Rate (per lane)
	BR
	
	53.125
	
	Gb/s
	

	Electrical Bit Error Rate (per lane)
	BER
	
	
	2.4E-4
	
	Notes


Notes: PRBS31Q@26.5625GBd. Pre-FEC



















LOW SPEED CONTROL AND SENSE SIGNALS
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DIGITAL DIAGNOSTIC SPECIFICATIONS
	Parameter
	Symbol
	Min
	Max
	Units
	Notes

	Transceiver case temperature accuracy
	DMI_TEMP
	-5
	+5
	℃
	Over operating temp

	Supply voltage monitor accuracy
	DMI _VCC
	-3%
	+3%
	V
	Full operating range

	Channel Bias current monitor accuracy
	DMI_IBIAS
	-10%
	+10%
	mA
	Per channel

	Channel RX power monitor absolute error
	DMI_RX
	-3
	3
	dB
	Per channel

	Channel TX power monitor absolute error
	DMI_TX
	-3
	3
	dB
	Per channel



OUTLINE DIAGRAM
 unit: mm
[image: ]
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