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FEATURES
· Compliant to QSFP28 Electrical MSA SFF-8636 Specification
· Wide Operating Temperature(0°C~70°C)
· 4x25Gbps 850nm VCSEL-based Transmitter
· RoHS compliant











APPLICATIONS

· 100GBASE-SR4 at 25.78125Gbps-28.05Gbps per lane
· InfiniBand QDR, EDR
· Other optical links


Ordering information
	Part Number
	Product Description

	JH-100G-QSFP28-A1-AOC
	100G QSFP28 AOC Transceivers, C-TEMP
xx=01~99,cable length=1m~99m
D1=100m





ABSOLUTE MAXIMUM RATINGS
	Parameter
	Symbol
	Conditions
	Min.
	Max.
	Unit

	Storage Temperature
	TStorage
	
	-40
	+85
	°C

	Relative Humidity
	RH
	
	0
	+85
	%




RECOMMENDED OPERATING CONDITIONS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Case Temperature
	TC
	
	0
	
	70
	°C

	Power Supply Voltage
	VCC
	
	3.135
	3.3
	3.465
	V

	Signaling Rate each Channel
	
	
	
	25.78125
	28.05
	Gbps

	Data Rate Accuracy
	
	
	-100
	
	100
	ppm

	Pre-FEC Bit Error Ratio 
	
	
	
	
	5e-5
	Note1

	Post-FEC Bit Error Ratio
	
	
	
	
	1e-12
	Note1



Notes1: FEC provided by host system.


ELECTRICAL CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Power Consumption
	
	
	
	
	2.5
	W

	Supply Current
	Icc
	
	
	
	750
	mA



PIN ASSIGNMENT  
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PIN DESCRIPTION  

	PIN
	Logic
	Symbol
	Name/Description
	Note

	1
	 
	GND
	Ground
	

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input
	

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data output
	

	4
	 
	GND
	Ground
	

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input
	

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data output
	

	7
	 
	GND
	Ground
	

	8
	LVTTL-I
	ModSelL
	Module Select
	

	9
	LVTTL-I
	ResetL
	Module Reset
	

	10
	 
	VccRx
	﹢3.3V Power Supply Receiver
	

	11
	LVCMOS-I/O
	SCL
	2-Wire Serial Interface Clock
	

	12
	LVCMOS-I/O
	SDA
	2-Wire Serial Interface Data
	

	13
	 
	GND
	Ground
	

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data Output
	

	15
	CML-O 
	Rx3n 
	Receiver Inverted Data Output 
	

	16
	 
	GND 
	Ground 
	

	17
	CML-O 
	Rx1p 
	Receiver Non-Inverted Data Output 
	

	18
	CML-O 
	Rx1n 
	Receiver Inverted Data Output 
	

	19
	 
	GND 
	Ground 
	

	20
	 
	GND 
	Ground 
	

	21
	CML-O 
	Rx2n 
	Receiver Inverted Data Output 
	

	22
	CML-O 
	Rx2p 
	Receiver Non-Inverted Data Output 
	

	23
	 
	GND 
	Ground 
	

	24
	CML-O 
	Rx4n 
	Receiver Inverted Data Output 
	

	25
	CML-O 
	Rx4p 
	Receiver Non-Inverted Data Output 
	

	26
	 
	GND 
	Ground 
	

	27
	LVTTL-O 
	ModPrsL 
	Module Present 
	

	28
	LVTTL-O 
	IntL 
	Interrupt 
	

	29
	 
	VccTx 
	+3.3 V Power Supply transmitter 
	

	30
	 
	Vcc1 
	+3.3 V Power Supply 
	

	31
	LVTTL-I 
	LPMode 
	Low Power Mode 
	

	32
	 
	GND 
	Ground 
	

	33
	CML-I 
	Tx3p 
	Transmitter Non-Inverted Data Input 
	

	34
	CML-I 
	Tx3n 
	Transmitter Inverted Data Output 
	

	35
	 
	GND 
	Ground 
	

	36
	CML-I 
	Tx1p 
	Transmitter Non-Inverted Data Input 
	

	37
	CML-I 
	Tx1n 
	Transmitter Inverted Data Output 
	

	38
	 
	GND 
	Ground 
	



Electrical Interface
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OUTLINE DIMENSIONS  
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Unit mm

Digital Diagnostic Monitor Accuracy
The following characteristics are defined over recommended operating conditions

	Parameter
	Accuracy
	Unit

	Internally measured transceiver temperature
	+/-3
	deg.C

	Internally measured transceiver supply voltage
	+/-3
	%

	Measured Tx bias current
	+/-10
	%

	Measured Tx output power
	+/-3
	dB

	Measured Rx received average optical power
	+/-3
	dB



Contact:
Wuhan Jiuhong Optics Technology Co., Ltd.
TEL: 86-13476016116
E-mail：grace@jh-optics.com
Web：www.jh-optics.com
Address：
Building 1, 4th Floor, Yunqi Free Trade Innovation Port, Donghu Comprehensive Bonded Zone,Donghu High-tech Zone, Wuhan City
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