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Product Specification
40Gb/s QSFP+ Active Optical Cable
                                 
1 Features 
· Supports 40G Ethernet interoperability
· Maximum link length of 70m links on OM3 multimode fiber or 100m links on OM4 multimode Fiber
· Electrically hot-pluggable
· Electrical interface compliant to QSFP+ connector 
· Case operating temperature range: 0°C to 70°C

2 Applications
· Network Switch Manufacturers supporting 40G 
· Server Manufacturers supporting 40G 

Ordering information
	Part Number
	Product Description

	JH-40G-QSFP+-A1-AOC
	40G QSFP+ to 40G QSFP+ Active Optical Cable Transceivers, C-TEMP
XX=01，cable length=1m
XX=03，cable length=3m
XX=05，cable length=5m
XX=0A，cable length=10m
XX=19，cable length=25m
XX=32，cable length=50m
XX=64，cable length=100m






3 General Description
This product QSFP+ to QSFP+ active optic cables are a high performance, low power consumption, long reach interconnect solution supporting 40G to 40G Ethernet.
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40G QSFP+

4 Pin Function Definition
[bookmark: _GoBack]Pin Definition- QSFP+
	PIN
	Logic
	Symbol
	Name/Description

	1
	
	GND
	Ground

	2
	CML-I
	Tx2n
	Transmitter Inverted Data Input

	3
	CML-I
	Tx2p
	Transmitter Non-Inverted Data output

	4
	
	GND
	Ground

	5
	CML-I
	Tx4n
	Transmitter Inverted Data Input

	6
	CML-I
	Tx4p
	Transmitter Non-Inverted Data output

	7
	
	GND
	Ground

	8
	[bookmark: OLE_LINK9][bookmark: OLE_LINK10]LVTLL-I
	ModSelL
	Module Select

	9
	LVTLL-I
	ResetL
	Module Reset

	10
	
	VccRx
	+3.3V Power Supply Receiver

	11
	LVCMOSS-I/O
	SCL
	2-Wire Serial Interface Clock

	12
	LVCMOSS-I/O
	SDA
	2-Wire Serial Interface Data

	13
	
	GND
	Ground

	14
	CML-O
	Rx3p
	Receiver Non-Inverted Data output

	15
	CML-O
	Rx3n
	Receiver Inverted Data Input

	16
	
	GND
	Ground

	17
	CML-O
	Rx1p
	Receiver Non-Inverted Data output

	18
	CML-O
	Rx1n
	Receiver Inverted Data Input

	19
	
	GND
	Ground

	20
	
	GND
	Ground

	21
	CML-O
	Rx2n
	Receiver Inverted Data Input

	22
	CML-O
	Rx2p
	Receiver Non-Inverted Data output

	23
	
	GND
	Ground

	24
	CML-O
	Rx4n
	Receiver Inverted Data Input

	25
	CML-O
	Rx4p
	Receiver Non-Inverted Data output

	26
	
	GND
	Ground

	27
	LVTLL-O
	ModPrsL
	Module Present

	28
	LVTLL-O
	IntL
	Interrupt

	29
	
	VccTx
	+3.3V Power Supply transmitter

	30
	
	Vccl
	+3.3V Power Supply

	31
	LVTLL-I
	LPMode
	Low Power Mode

	32
	
	GND
	Ground

	33
	CML-I
	Tx3p
	Transmitter Non-Inverted Data output

	34
	CML-I
	Tx3n
	Transmitter Inverted Data Input

	35
	
	GND
	Ground

	36
	CML-I
	Tx1p
	Transmitter Non-Inverted Data output

	37
	CML-I
	Tx1n
	Transmitter Inverted Data Input

	38
	
	GND
	Ground
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5 Recommended Power Supply Filter
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6 Performance Specifications
6.1 Absolute Maximum Ratings
It has to be noted that the operation in excess of any individual absolute maximum ratings might cause permanent damage to this module
	Parameter
	Symbol
	Min.
	Max.
	Unit

	Storage Temperature
	Tstg
	-40
	+85
	[bookmark: OLE_LINK11][bookmark: OLE_LINK12]°C

	Operating relative humidity
(Non- condensing)
	RH
	0
	85
	%

	Input Voltage
	
	Vcc-0.3
	Vcc+0.3
	V

	Supply Voltage
	Vcc
	-0.3
	3.6
	dBm



6.2 Recommended Operating Conditions and Power Supply Requirements
	[bookmark: _Hlk509495219][bookmark: OLE_LINK13][bookmark: OLE_LINK14]Parameter
	Symbol
	Min.
	Type
	Max.
	Unit
	NOTE

	[bookmark: _Hlk496606561][bookmark: OLE_LINK2][bookmark: OLE_LINK1]Operating Case Temperature
	[bookmark: OLE_LINK17][bookmark: OLE_LINK16]Tc
	0
	
	+70
	℃
	

	Power Supply Voltage
	Vcc
	+3.135
	3.3
	+3.465
	V
	

	Data Rate
	BR
	
	41.25
	
	Gb/s
	QSFP+ Bit Rate

	Power Consumption Max (per cable)
	P
	
	
	2.5
	W
	End-QSFP+

	Supply Current (per cable)
	ICC
	
	
	0.76
	A
	End-QSFP+

	Data Rate Accuracy
	-
	-100
	
	100
	ppm
	

	Control Input Voltage High 
	-
	-
	
	2
	V
	

	Control Input Voltage Low
	-
	0.8
	
	-
	V
	

	Link Distance(OM4 MMF)
	D
	0
	
	100
	m
	



6.3 Electrical Specification
	Parameter
	Symbol
	Min.
	Typ.
	Max.
	Unit

	Differential input impedance
	Zin
	90
	100
	110
	ohm

	Differential Output impedance
	Zout
	90
	100
	110
	ohm

	Differential input voltage amplitude
	ΔVin
	300
	
	1100
	mVp-p

	Differential output voltage amplitude
	ΔVout
	500
	
	800
	mVp-p

	Bit Error Ratio
	BR
	
	
	1E-12

	Input Logic Level High
	VIH
	2.0
	
	VCC
	V

	Input Logic Level Low
	VIL
	0
	
	0.8
	V

	Output Logic Level High
	VOH
	VCC-0.5
	
	VCC
	V

	Output Logic Level Low
	VOL
	0
	
	0.4
	V












7 Mechanical Dimensions
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40G QSFP+

(Unit: mm)

8 Digital Diagnostic Monitor Accuracy
The following characteristics are defined over recommended operating conditions
	Parameter
	Accuracy
	Unit

	Internally measured transceiver temperature
	+/-3
	deg.C

	Internally measured transceiver supply voltage
	+/-3
	%

	Measured Tx bias current
	+/-10
	%

	Measured Tx output power
	+/-3
	dB

	Measured Rx received average optical power
	+/-3
	dB
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Figure 3. Recommended Power Supply Filter
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