Product Specification
16GFC SFP+ SR Dual LC Transceivers

 
PRODUCT FEATURES 
· 16GFC(14.025Gb/s) serial optical interface 
· 850nm VCSEL transmitter and GaAs PIN PD receiver
· Wide operating temperature(0°C~70°C)
· Low power consumption <1W
· Maximum link length of 70m via OM3 multimode Fiber (MMF)
· Maximum link length of 100m via OM4 multimode Fiber (MMF)
·  Fibre Channel FC-PI-6 compliant high speed interface
--3200-M5-SN-S, 3200-M5E-SN-I, 3200-M5F-SN-I

Application
· Fibre Channel switches (director, stand alone, blade)
· Fibre Channel Host Bus Adapters
· Fibre Channel RAID controllers
· Fibre Channel tape drive
· Port side connections
· Inter-switch or inter-chassis aggregated links
Ordering information
	Part Number
	Product Description

	JH-16G-SFP+-SR
	16GFC SFP+ SR Transceivers, C-TEMP



DESCRIPTION
The 16GFC SFP+ SR Transceiver is intended for 100m reach service 14.025Gb/s 850nm Multi-mode high-speed communications equipment where low-cost, extraordinary performance and reliability are essential. It consumes low power, operates base on 3.3V DC power supply and is offered in the commercial temperature range. They are compliant with SFP+ MSA, SFF-8431 and SFF-8432.  High speed electrical and optical specifications are compliant with ANSI Fibre Channel FC-PI-6.

 The 16GFC SFP+ is a multi-rate 850nm transceiver which ensures compliance with 16GFC specifications. Per the requirements of 16GFC, internal clock and data recovery circuits (CDRs) are present on both electrical input and electrical output of this transceiver for low jitter compliance. 
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ABSOLUTE MAXIMUM RATINGS
	Parameter
	Symbol
	Conditions
	Min.
	Max.
	Unit

	Storage Temperature
	TStorage
	
	-40
	+85
	°C

	Relative Humidity
	RH
	
	0
	+85
	%





RECOMMENDED OPERATING CONDITIONS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Case Temperature
	TC
	
	0
	
	70
	°C

	Power Supply Voltage
	VCC
	
	3.15
	3.3
	3.45
	V

	Signaling Rate each Channel
	
	
	
	[bookmark: _GoBack]14.025
	
	Gbps





ELECTRICAL CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Power Consumption
	
	
	
	
	1
	W

	Supply Current
	Icc
	
	
	
	300
	mA





TRANSMITTER CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Center wavelength
	λ
	
	840
	
	860
	nm

	RMS spectral width
	Pm
	
	
	
	0.6
	nm

	Average optical power
	Pavg
	
	-8.4
	
	2.4
	dBm

	Optical modulation amplitude
	OMA
	
	-6.4
	
	3
	dBm

	Average launch power of OFF transmitter
	Poff
	
	
	
	-30
	dBm

	Extinction ratio
	ER
	
	2
	
	
	dB

	Optical return loss tolerance
	
	
	
	
	12
	dB
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RECEIVER CHARACTERISTICS (T=25°C, unless noted)
	Parameter
	Symbol
	Conditions
	Min.
	Typ.
	Max.
	Unit

	Center wavelength
	λ
	
	840
	850
	860
	nm

	Damage threshold
	
	
	3.4
	
	
	dBm

	Receive power overload 
	
	
	2.4
	
	
	dBm

	Receiver reflectance
	
	
	
	
	-12
	dB

	Receiver sensitivity
	SENS
	
	
	
	-10
	dBm

	LOS Assert 
	LOSA
	
	-30
	
	
	dBm

	LOS De-Assert 
	LOSD
	
	
	
	-13
	dBm

	LOS Hysteresis
	LOSH
	
	0.5
	
	
	dB



PIN ASSIGNMENT  

[image: ]


PIN DESCRIPTION  
[image: ]


Recommended Interface Circuit
[image: ]
Figure 2. Typical application circuit











Mechanical Dimensions
[image: ]
Figure 3. Module Mechanical Dimensions

Digital Diagnostics Functions
As defined by the SFF-8472, Our SFP+ transceivers provide digital diagnostic functions via a 2-wire serial interface, which allows real-time access to the following operating parameters:
· Transceiver temperature
· Laser bias current
· Transmitted optical power
· Received optical power
· Transceiver supply voltage
It also provides a sophisticated system of alarm and warning flags, which may be used to alert end-users when particular operating parameters are outside of a factory-set normal range. The operating and diagnostics information is monitored and reported by a Digital Diagnostics Transceiver Controller (DDTC) inside the transceiver, which is accessed through the 2-wire serial interface. The memories are organized as a series of 8-bit data words that can be addressed individually or sequentially. The 2-wire serial interface provides sequential or random access to the 8 bit parameters, addressed from 0x00h to the maximum address of the memory. For more detailed information, including memory map definitions, please refer the SFF-8472 documentation. 


Digital Diagnostic Monitor Accuracy
The following characteristics are defined over recommended operating conditions

	Parameter
	Accuracy
	Unit

	Internally measured transceiver temperature
	+/-3
	deg.C

	Internally measured transceiver supply voltage
	+/-3
	%

	Measured Tx bias current
	+/-10
	%

	Measured Tx output power
	+/-3
	dB

	Measured Rx received average optical power
	+/-3
	dB




Contact:
Wuhan Jiuhong Optics Technology Co., Ltd.
TEL: 86-13476016116
E-mail：grace@jh-optics.com
Web：www.jh-optics.com
Address：Building 1, 4th Floor, Yunqi Free Trade Innovation Port, Donghu Comprehensive Bonded Zone,Donghu High-tech Zone, Wuhan City


3pecifications are subject to change without notice.		Version 2.1        2/3
image5.png
8
bt

® 6,25¢0,05—

4,70£0,05 @

O@u a0 5 @L702015 — — 1728015 —13,90£0,1
o # e
g n I_H_E
7 |e 9| LT
imjs m oty
f 7 ﬁ
0,60%0,1( = A Al
0 0 ® -
g 4 —
g Y g
g 38
2 m 5 8,550,106
2 0B ®
®13,70£0,10- =
E ®2,2540,10+
@ 1,00£0,10-

©13,50 4

@2.00£0,15+





image2.emf

image3.emf

image4.png
ot o

= e
w

R nfw

Rl I N S

| , Protocol
e = ‘l:
el
J— o= s





image1.jpeg
Optoelectronic




